|  |
| --- |
| ./not\_causal.out 9094 9095 9096 |
|  | Buffer content sending is:10 9094 |
|  |  |
|  | Port of sender is:9094 |
|  |  |
|  | Received message 6 from 9094 port |
|  |  |
|  | Buffer content sending is:11 9095 |
|  |  |
|  | Port of sender is:9095 |
|  |  |
|  | Received message 11 from 9094 port |
|  |  |
|  | Buffer content sending is:12 9096 |
|  |  |
|  | Port of sender is:9096 |
|  |  |
|  | Received message 12 from 9094 port |
|  |  |
|  |  |